Test p13

1-

a- input ports

b- output ports

c- switching fabric

d- routing processor

2-

a- fiber cable

b- coaxial cable

3- colleges

4- to break a LAN into segments to relieve traffic congestion