Test

Q1.

 Input ports

Output ports

A switching fabric

A routing processor

Q2.

Coaxial twisted pair

Fiber \_optic cabling

Q3.

Outside plant

Campus network in building and the horizontal

Q4

To break a LAN into segments to relieve traffic congestion